
# XFree86 4 configuration created by pyxf86config

Section "ServerLayout"
	Identifier     "Default Layout"
	Screen      0  "Screen0" 0 0
	InputDevice    "Mouse0" "CorePointer"
	InputDevice    "Keyboard0" "CoreKeyboard"
	InputDevice    "Penmount" "AlwaysCore"
EndSection

Section "Files"

# RgbPath is the location of the RGB database.  Note, this is the name of the 
# file minus the extension (like ".txt" or ".db").  There is normally
# no need to change the default.
# Multiple FontPath entries are allowed (they are concatenated together)
# By default, Red Hat 6.0 and later now use a font server independent of
# the X server to render fonts.
	RgbPath      "/usr/X11R6/lib/X11/rgb"
	FontPath     "unix/:7100"
EndSection

Section "Module"
	Load  "dbe"
	Load  "extmod"
	Load  "fbdevhw"
	Load  "glx"
	Load  "record"
	Load  "freetype"
	Load  "type1"
	Load  "dri"
EndSection

Section "InputDevice"

# Specify which keyboard LEDs can be user-controlled (eg, with xset(1))
#	Option	"Xleds"		"1 2 3"
# To disable the XKEYBOARD extension, uncomment XkbDisable.
#	Option	"XkbDisable"
# To customise the XKB settings to suit your keyboard, modify the
# lines below (which are the defaults).  For example, for a non-U.S.
# keyboard, you will probably want to use:
#	Option	"XkbModel"	"pc102"
# If you have a US Microsoft Natural keyboard, you can use:
#	Option	"XkbModel"	"microsoft"
#
# Then to change the language, change the Layout setting.
# For example, a german layout can be obtained with:
#	Option	"XkbLayout"	"de"
# or:
#	Option	"XkbLayout"	"de"
#	Option	"XkbVariant"	"nodeadkeys"
#
# If you'd like to switch the positions of your capslock and
# control keys, use:
#	Option	"XkbOptions"	"ctrl:swapcaps"
# Or if you just want both to be control, use:
#	Option	"XkbOptions"	"ctrl:nocaps"
#
	Identifier  "Keyboard0"
	Driver      "kbd"
	Option	    "XkbModel" "pc105"
	Option	    "XkbLayout" "us"
EndSection

Section "InputDevice"
	Identifier  "Mouse0"
	Driver      "mouse"
	Option	    "Protocol" "IMPS/2"
	Option	    "Device" "/dev/input/mice"
	Option	    "ZAxisMapping" "4 5"
	Option	    "Emulate3Buttons" "yes"
EndSection

Section "InputDevice"
	Identifier  "PenMount"
	Driver      "penmount"
	Option      "Protocol"	   "Auto"
	Option      "Device"	   "/dev/ttyS0"  #ttys0=COM1,ttys1=COM2
	Option      "PMode"        "1"
	Option	    "MinX"	   "10"
	Option	    "MaxX"	   "1000"
	Option	    "MinY"	   "10"
	Option	    "MaxY"	   "1000"
        Option      "Beep"         "1"	    #  0 = no beep, 1 = beep enabled
        Option      "PressVol"     "100"    #  volume of beep (press event)
        Option      "PressPitch"   "880"    #  pitch of beep (press event)
        Option      "PressDur"     "15"     #  length of beep in 10ms (press event)
        Option      "ReleaseVol"   "0"	    #  volume of beep (release event)
        Option      "ReleasePitch" "1200"   #  pitch of beep (release event) 
        Option      "ReleaseDur"   "10"	    #  length of beep in 10ms (release event)
	Option	    "BaudRate"     "19200"  #  or "9600" (baud rate of serial port)
EndSection

Section "Monitor"
	Identifier   "Monitor0"
	VendorName   "Monitor Vendor"
	ModelName    "150B"
	DisplaySize  300	230
	HorizSync    30.0 - 61.0
	VertRefresh  56.0 - 75.0
	Option	    "dpms"
EndSection

Section "Device"
	Identifier  "Videocard0"
	Driver      "vesa"
	VendorName  "Videocard vendor"
	BoardName   "Trident CyberBlade (generic)"
EndSection

Section "Screen"
	Identifier "Screen0"
	Device     "Videocard0"
	Monitor    "Monitor0"
	DefaultDepth     24
	SubSection "Display"
		Viewport   0 0
		Depth     16
		Modes    "800x600" "640x480"
	EndSubSection
	SubSection "Display"
		Viewport   0 0
		Depth     24
		Modes    "1024x768" "800x600" "640x480"
	EndSubSection
EndSection

Section "DRI"
	Group        0
	Mode         0666
EndSection

